
V1.1.2/2014-01-16
Please be noted, you need to update both the firmware and the config file to both Tx and rx.
	
What's new?

1:Add micro power mode for range check
2:Add PPM random mapping and PWM channels random mapping, and they are totally independent, which means you can map PPM output to chan1-chan8, and map PWM1-PWM8 output 
to be chan9-chan16.
3:Add and test communication code with Rlink Companion.
4:Add low and high power voltage warning configurable option.
5:Avoid wrong warning of PPM input check.
6:Add can-bus communication code with R2M OSD module
7:Add protection login for failsafe setting, you need to press the FS button for over 1s to transmit one time of failsafe positions,avoid wrong operation
8:Add config file error indicator for both Tx and Rx
  Tx: the red LED on the top will flash one long time, and 2 short time, buzzor will beep as"Di-----Di-----Di"
  Rx: the red LED will flash one long time, and 2 short time.
9:fix the bug that you can't switch the RSSI output based on RSSI or package right rate when the Rx doesn't receive data. and change the indicator, red led: right packat rate, blue: RSSI
10:Change the logic of bind for adding micro power mode for Tx:
Holding the FS button, switch to low power mode, and power on the Tx, there will be a long beep which indicate to enter micro power mode
Holding the FS button, switch to High power mode, and power on the Tx, the Tx enter binding mode.


   
   
   
	