
**Jumper FPV Headband display**

JP-VR7 FPV Headband display is designed for FPV crossing design, using ultra-low latency of 800 \* 480 screen, with the grading receiving module, image signal a more direct and more smoothly.



Display Specifications

Resolution：800\*480

Perspective：70°

Dial-up menus to adjust

Screen Delay ：5ms

Basic Specifications Features

Dial buttons

Adjustable elastic energy

Power input

Power consumption：300ma@12v

Operating Voltage：7-25v（2s-6s）

RF Receiver

40-channel receiver grading 5.8g

(double receiver module)

